(footprint "C_0402_1005Metric" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5F68FEEE)
  (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
  (tags "capacitor")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.16) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 480a46d7-23ef-4741-81b5-dbf347b86fdb)
  )
  (fp_text value "1uF" (at 0 1.16) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a3b11e5d-b404-4199-a5c2-6236c4c4896f)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 0.25 0.25) (thickness 0.04)))
    (tstamp 07358330-0b2c-4c48-8b11-1f588b07df1b)
  )
  (fp_line (start -0.107836 0.36) (end 0.107836 0.36) (layer "F.SilkS") (width 0.12) (tstamp 84193a0f-7546-438a-88f3-df18874a34d8))
  (fp_line (start -0.107836 -0.36) (end 0.107836 -0.36) (layer "F.SilkS") (width 0.12) (tstamp 8d7db1ec-fc6c-445e-bdef-bbf4efe3e629))
  (fp_line (start 0.91 0.46) (end -0.91 0.46) (layer "F.CrtYd") (width 0.05) (tstamp 1710bf04-ed4b-466c-b4a7-c22c721f96c1))
  (fp_line (start -0.91 -0.46) (end 0.91 -0.46) (layer "F.CrtYd") (width 0.05) (tstamp 1b5031c8-9684-49cf-a045-a3f60458b44a))
  (fp_line (start -0.91 0.46) (end -0.91 -0.46) (layer "F.CrtYd") (width 0.05) (tstamp 85aaf66d-3204-45c7-a6df-2b79623b57cd))
  (fp_line (start 0.91 -0.46) (end 0.91 0.46) (layer "F.CrtYd") (width 0.05) (tstamp 9f276897-97e9-4b1d-9f0d-1678a783b6a1))
  (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer "F.Fab") (width 0.1) (tstamp 33a5ec73-41aa-47d0-aad8-ca980947ea5b))
  (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer "F.Fab") (width 0.1) (tstamp 3bec72ec-6d3e-4707-9797-5664bc83ca95))
  (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer "F.Fab") (width 0.1) (tstamp 726b90f0-d3ec-406b-a446-2ef5c3227f25))
  (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer "F.Fab") (width 0.1) (tstamp b79be662-d484-4294-abf3-88d38a801efb))
  (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 979131b8-4334-4a66-95d4-d4f722f7c2b9))
  (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 80c36828-7c6b-4966-8ed2-c6a48ed2c92f))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
