(footprint "UNBProbe_Castellated_Pad" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6054B15A)
  (descr "SMD rectangular pad as test Point, square 1.0mm side length")
  (tags "test point SMD pad rectangle square")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a3645da2-be87-4361-8567-4663dc46954b)
  )
  (fp_text value "UNBProbe_Castellated_Pad" (at 0 1.55) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7fc7b070-19a0-47c2-bcde-ad8ad148b96e)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 525562d5-bfdd-45a7-9302-02f18adfa7c2)
  )
  (fp_line (start 1 1) (end 1 -1.78308) (layer "F.CrtYd") (width 0.05) (tstamp 2caf766b-7382-4261-8c22-a99aceda4c99))
  (fp_line (start -1 -1.78308) (end 1 -1.78308) (layer "F.CrtYd") (width 0.05) (tstamp 8b15caf5-8141-426c-aad1-fb2ccd5a4a60))
  (fp_line (start -1 -1.78308) (end -1 1) (layer "F.CrtYd") (width 0.05) (tstamp e9727c22-06b7-4a6c-9802-4bd3a4416044))
  (fp_line (start 1 1) (end -1 1) (layer "F.CrtYd") (width 0.05) (tstamp fb0c3bca-c014-4bfb-bfaa-a843cc148a6b))
  (pad "1" thru_hole rect (at 0 0) (size 0.8 1.5) (drill 0.6 (offset 0 -0.375)) (property pad_prop_castellated) (layers *.Cu *.Mask) (tstamp 89e97a1a-b91c-4fff-9881-27bdea08aa86))
)
