(footprint "PinHeader_1x01_P2.54mm_Vertical_SilkAlter" (version 20211014) (generator pcbnew)
  locked (layer "F.Cu")
  (tedit 609F7651)
  (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x01 2.54mm single row")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -2.33) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d9a76eb7-53c8-4881-9e9e-bafb83b84c81)
  )
  (fp_text value "PinHeader_1x01_P2.54mm_Vertical_SilkAlter" (at 0 2.33) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b771fb66-f1f1-4c2a-a8ce-4548f8644210)
  )
  (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp babdc19d-650f-44db-839b-fc9b26091cc8)
  )
  (fp_line (start -1.33 1.31) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 47429d92-6cdd-47bd-92f9-38748d372703))
  (fp_line (start 1.33 -1.33) (end 1.33 1.31) (layer "F.SilkS") (width 0.12) (tstamp 4891c9e2-49f9-43eb-9081-14ab045a4fd1))
  (fp_line (start -1.33 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 8d9d9155-f082-4462-8803-ec255a04cbdc))
  (fp_line (start 1.33 1.31) (end -1.33 1.31) (layer "F.SilkS") (width 0.12) (tstamp aab7f528-3165-4da9-b5f9-443b631ec8ce))
  (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer "F.CrtYd") (width 0.05) (tstamp 2aba7061-249c-4994-98f2-dc0bbecf125b))
  (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 6c859158-1d42-4163-9d71-aa0bf33c16c6))
  (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer "F.CrtYd") (width 0.05) (tstamp 74a4ae30-4bd3-47af-992d-daab0d9bf2ea))
  (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp fb76070e-e799-46bc-9274-737f33052172))
  (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 2d004d4b-e8df-4d94-bbe0-b25f97326031))
  (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 5d2fb743-7a32-4277-a23a-910e06a720e8))
  (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp a3c63c26-ae2e-4e85-afb5-78829ad505a9))
  (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp a6c6b594-cf3c-4a5f-8bb5-ae67b5fea4ed))
  (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp ab0f969d-9080-4508-a70b-293d852551ee))
  (pad "17" thru_hole rect locked (at 0 -0.000164) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
    (zone_connect 2) (tstamp cc7d2b79-c988-4ea7-8fd2-7ccfc4116839))
  (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
