(footprint "SMA_Amphenol_901-144_Vertical" (version 20211014) (generator pcbnew)
  locked (layer "F.Cu")
  (tedit 5B2F4C32)
  (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
  (tags "SMA THT Female Jack Vertical")
  (attr through_hole)
  (fp_text reference "REF**" (at 6.084 3.68) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cc22344d-dcad-4daa-8ffe-5917207c8176)
  )
  (fp_text value "Conn_Coaxial" (at 0 5) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 77165e27-ace7-4971-bd71-9a6081fe51ed)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9d315973-459f-4c77-ba69-41c2e532d7a8)
  )
  (fp_line (start 3.355 -1.45) (end 3.355 1.45) (layer "F.SilkS") (width 0.12) (tstamp 047c290c-c270-4a1e-bba9-09bb1d99812c))
  (fp_line (start -3.355 -1.45) (end -3.355 1.45) (layer "F.SilkS") (width 0.12) (tstamp 2ee1e621-8a60-4501-8e57-86cea014e6e5))
  (fp_line (start -1.45 -3.355) (end 1.45 -3.355) (layer "F.SilkS") (width 0.12) (tstamp 6d7d47b7-2a86-473d-b1ce-7a34f2d80d64))
  (fp_line (start -1.45 3.355) (end 1.45 3.355) (layer "F.SilkS") (width 0.12) (tstamp 83f1019b-2285-47d9-8786-f6a337046a5e))
  (fp_line (start -4.17 -4.17) (end 4.17 -4.17) (layer "F.CrtYd") (width 0.05) (tstamp 15428b7e-1c96-40b0-be6e-764b9d4303f4))
  (fp_line (start 4.17 4.17) (end 4.17 -4.17) (layer "F.CrtYd") (width 0.05) (tstamp 432dd1d6-7b6d-466d-b774-8045ff408a0d))
  (fp_line (start 4.17 4.17) (end -4.17 4.17) (layer "F.CrtYd") (width 0.05) (tstamp 7f84f3a4-26da-4fa5-8b57-ba74e7ee99e1))
  (fp_line (start -4.17 -4.17) (end -4.17 4.17) (layer "F.CrtYd") (width 0.05) (tstamp a5b22fb1-e5d9-48e9-a483-2cae18be29fd))
  (fp_line (start 3.175 -3.175) (end 3.175 3.175) (layer "F.Fab") (width 0.1) (tstamp 27bff318-9e84-400e-90e7-6ae4f53830f4))
  (fp_line (start -3.175 3.175) (end 3.175 3.175) (layer "F.Fab") (width 0.1) (tstamp 337e38d5-2434-491c-b615-1f2ed1a6a72e))
  (fp_line (start -3.175 -3.175) (end -3.175 3.175) (layer "F.Fab") (width 0.1) (tstamp 7c58b13f-7be4-4197-b5ce-9c6ea92361c2))
  (fp_line (start -3.175 -3.175) (end 3.175 -3.175) (layer "F.Fab") (width 0.1) (tstamp 9930fa14-c8ac-4aa1-a31a-4fe28fb7f45e))
  (fp_circle (center 0 0) (end 3.175 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 16344f9a-2032-4a81-845a-78bebdd6e51f))
  (pad "1" thru_hole circle locked (at 0 0) (size 2.05 2.05) (drill 1.5) (layers *.Cu *.Mask) (tstamp beab38eb-50be-42db-97ba-36e41dac61b7))
  (pad "2" thru_hole circle locked (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask) (tstamp 07dd8b9d-bc45-467e-a21d-b167811a119b))
  (pad "2" thru_hole circle locked (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask) (tstamp 68b350a2-c0ea-477c-b896-2e609c324a28))
  (pad "2" thru_hole circle locked (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask) (tstamp 899faf3f-3555-483c-9043-f7f9a5f25562))
  (pad "2" thru_hole circle locked (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask) (tstamp b0dda047-f4cd-4c48-88dd-5c257468d748))
  (model "${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KIPRJMOD}/3dmodels/2985-6004--3DModel-STEP-1.STEP"
    (offset (xyz 0 0 9.6))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
