(footprint "PinHeader_1x12_P2.54mm_Vertical_AlteredSilk" (version 20211014) (generator pcbnew)
  locked (layer "F.Cu")
  (tedit 609F7162)
  (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x12 2.54mm single row")
  (attr through_hole)
  (fp_text reference "REF**" (at 3.433 0.003 -180) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ef667ece-1f0c-452e-bcec-e837a29274a5)
  )
  (fp_text value "Conn_01x12" (at -4.425 0.915 90) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a3fbbb32-7916-4a55-841f-36c3acc16d86)
  )
  (fp_text user "${REFERENCE}" (at 0 13.97 -90) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 334ef330-8856-4296-94a3-f6aa921877ac)
  )
  (fp_line (start -1.33 -1.33) (end -1.33 29.27) (layer "F.SilkS") (width 0.12) (tstamp 0073cd7d-67b2-4b8e-95b2-e363918496bb))
  (fp_line (start 1.33 -1.33) (end 1.33 29.27) (layer "F.SilkS") (width 0.12) (tstamp 780a8bdb-d3f2-4ccb-ad9d-6abfe5aa6a04))
  (fp_line (start -1.33 29.27) (end 1.33 29.27) (layer "F.SilkS") (width 0.12) (tstamp 9375ab3f-0eac-40e1-8b80-ea1d54cfb7de))
  (fp_line (start -1.33 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp dfa5674e-6fb9-4aea-b6b9-fe87312bf31a))
  (fp_line (start 1.8 29.75) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 37e437e9-21b3-4fda-adf3-974141205146))
  (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 93294809-3473-44c1-96c6-f6f680ca3e6d))
  (fp_line (start -1.8 -1.8) (end -1.8 29.75) (layer "F.CrtYd") (width 0.05) (tstamp b615ea4c-4a7c-47f9-9e24-078b5f8fc285))
  (fp_line (start -1.8 29.75) (end 1.8 29.75) (layer "F.CrtYd") (width 0.05) (tstamp ba31bf85-25d0-4187-9e3c-7f27d066da7c))
  (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 07e4a594-198c-472c-951b-31964d592c37))
  (fp_line (start 1.27 -1.27) (end 1.27 29.21) (layer "F.Fab") (width 0.1) (tstamp 0bf290dd-2ef7-4404-ba2c-be18aecf6c80))
  (fp_line (start -1.27 29.21) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 33dcd407-a68b-4b6a-8cb5-84bac1705ec3))
  (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 957eb1e6-fbf7-4735-90d5-52e84096e3ca))
  (fp_line (start 1.27 29.21) (end -1.27 29.21) (layer "F.Fab") (width 0.1) (tstamp 9a2013ad-47c0-4be8-8352-d8a7c3f743fb))
  (pad "1" thru_hole circle locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 07fb19ce-037f-42cd-ac8f-fb60b6189d32))
  (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp d651fe81-b03a-4ed5-bed5-e3b68af83cb6))
  (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 3fd5b823-2a77-4012-a651-3c786de94282))
  (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 68c84021-827d-4bc8-8599-14168d974692))
  (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 40532640-b8b4-46f2-8284-f1040993bbb2))
  (pad "6" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp f16e0064-1951-4925-b2e3-592d1404d892))
  (pad "7" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp f5df6ede-638c-4cd4-b02d-b741f8f56d32))
  (pad "8" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 88546f85-0a77-407d-9262-9012d85a4200))
  (pad "9" thru_hole oval locked (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp ec257a5d-6a92-41c6-a331-8903420f996a))
  (pad "10" thru_hole oval locked (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 2d8b9a7c-d043-4c33-853d-28b004ac95cc))
  (pad "11" thru_hole oval locked (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp c4a41119-c259-460e-88c4-c45dcf49c2ae))
  (pad "12" thru_hole oval locked (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 9dcee99a-6978-401e-844d-fe920febdb77))
  (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
