%TF.GenerationSoftware,KiCad,Pcbnew,6.0.11+dfsg-1*%
%TF.CreationDate,2025-11-09T17:51:53+01:00*%
%TF.ProjectId,UNBProbe,554e4250-726f-4626-952e-6b696361645f,0.3*%
%TF.SameCoordinates,Original*%
%TF.FileFunction,Soldermask,Bot*%
%TF.FilePolarity,Negative*%
%FSLAX46Y46*%
G04 Gerber Fmt 4.6, Leading zero omitted, Abs format (unit mm)*
G04 Created by KiCad (PCBNEW 6.0.11+dfsg-1) date 2025-11-09 17:51:53*
%MOMM*%
%LPD*%
G01*
G04 APERTURE LIST*
G04 Aperture macros list*
%AMHorizOval*
0 Thick line with rounded ends*
0 $1 width*
0 $2 $3 position (X,Y) of the first rounded end (center of the circle)*
0 $4 $5 position (X,Y) of the second rounded end (center of the circle)*
0 Add line between two ends*
20,1,$1,$2,$3,$4,$5,0*
0 Add two circle primitives to create the rounded ends*
1,1,$1,$2,$3*
1,1,$1,$4,$5*%
%AMRotRect*
0 Rectangle, with rotation*
0 The origin of the aperture is its center*
0 $1 length*
0 $2 width*
0 $3 Rotation angle, in degrees counterclockwise*
0 Add horizontal line*
21,1,$1,$2,0,0,$3*%
G04 Aperture macros list end*
%ADD10HorizOval,1.700000X0.000000X0.000000X0.000000X0.000000X0*%
%ADD11RotRect,1.700000X1.700000X45.000000*%
%ADD12R,1.500000X0.800000*%
%ADD13R,0.800000X1.500000*%
G04 APERTURE END LIST*
D10*
%TO.C,J2*%
X164606518Y-102424011D03*
D11*
X166402569Y-104220062D03*
%TD*%
D12*
%TO.C,P1*%
X124156518Y-101632011D03*
%TD*%
D13*
%TO.C,REF\u002A\u002A*%
X115841518Y-102486611D03*
%TD*%
%TO.C,REF\u002A\u002A*%
X121841518Y-100776411D03*
%TD*%
%TO.C,REF\u002A\u002A*%
X118841518Y-102486611D03*
%TD*%
%TO.C,REF\u002A\u002A*%
X115841518Y-100786411D03*
%TD*%
%TO.C,REF\u002A\u002A*%
X121841518Y-102486611D03*
%TD*%
%TO.C,REF\u002A\u002A*%
X118841518Y-100776411D03*
%TD*%
M02*
