(footprint "MountingHole_2.2mm_M2_ISO7380_Pad" (version 20211014) (generator pcbnew)
  locked (layer "F.Cu")
  (tedit 609E6B64)
  (descr "Mounting Hole 2.2mm, M2, ISO7380")
  (tags "mounting hole 2.2mm m2 iso7380")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -2.75) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 505a7c59-577d-4262-8bcf-d22518721feb)
  )
  (fp_text value "MountingHole_2.2mm_M2_ISO7380_Pad" (at 0 2.75) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 22222fbf-1ac5-48b1-8009-38372eedceef)
  )
  (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 39e9695c-c1df-4807-87d8-8e6f7a141f9a)
  )
  (fp_circle (center 0 0) (end 1.75 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp db23d2b3-9e22-4f77-be9f-33cce77ae310))
  (fp_circle (center 0 0) (end 2 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 4d80af86-ef83-4a04-b1f6-c3f6d3413947))
  (pad "16" thru_hole circle locked (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask) (tstamp 6a7f30cf-99eb-4b20-b292-49263878ebf6))
)
